[GENERAL]
delmsg1=delete all readings ?
emptyMsg=memory empty
endmsg=please end continuous measurement first
luxmsg=iluminance [lx]
fcmsg=illuminance [fc]
lumiMsg=luminance [cd/mē]
lumiMsg2=luminance [ftLb]
MemDelMsg=the memory has been cleared
mval=value
readMsg= readings read from memory
relmsg=loose all readings ?
relmsg2=reject all readings ?
meamsg1=continuous mode off
meamsg2=continuous mode on


[DefaultBtns]
AbortBtn=&Abort
AllBtn=&All
CloseBtn=&Close
CancelBtn=&Cancel
HelpBtn=&Help
IgnoreBtn=&Ignore
NoBtn=&No
OKBtn=&OK
RetryBtn=&Retry
YesBtn=&Yes

[DefaultDlgs]
Confirmation=confirmation
Error=error
warning=warning
Info=info

